1ANSI X3.210A-199xSupplement to ANSI X3.210-1992American National Standardfor information systems —supplement to High-Performance Parallel Interface —Framing Protocol (HIPPI-FP)Approved ????, 199xSecretariat: Computer Business EquipmentManufacturers AssociationPage 1 of 2 pagesAmendments to ANSI X3.210-1992On page v,delete lines 19 through 28, i.e., from "The information in this document..." through "Clause 7specifies the data, header, and packet formats."On page v,replace figure 1 with the following figure. HIPPI-LELink EncapsulationMechanical, Electrical, and SignallingProtocol HIPPI-PH(physical layer) HIPPI-SCSwitch Control(control of HIPPI physical layer switches)(mapping to IEEE 802.2) HIPPI-FC IPI-3 Disk(mapping to FibreChannel ULP’s) IPI-3 Tape HIPPI-FP(generic disk command set)(generic tape command set)Framing ProtocolFigure 1 — HIPPI-FP relationship to other entitiesAn American National Standard implies a consensus of those substantially concerned with its scope and provisions. An American NationalStandard is intended as a guide to aid the manufacturer, the consumer, and the general public. The existence of an American NationalStandard does not in any respect preclude anyone, whether he has approved the standard or not, from manufacturing, marketing,purchasing, or using products, processes, or procedures not conforming to the standard. American National Standards are subject toperiodic review and users are cautioned to obtain the latest editions.The American National Standards Institute does not develop standards and will in no circumstances give an interpretation of any AmericanNational Standard. Moreover, no person shall have the right or authority to issue an interpretation of an American National Standard in thename of the American National Standards Institute.CAUTION NOTICE: This American National Standard may be revised or withdrawn at any time. The procedures of the American NationalStandards Institute require that action be taken to reaffirm, revise, or withdraw this standard no later than five years from the date ofapproval. Purchasers of American National Standards may receive current information on all standards by calling or writing the AmericanNational Standards Institute.

2Page 2 of 2On page 4,replace the list of ULP identifiers in 5.4.1 with:00000010 = Reserved00000011 = Reserved00000100 = ISO 8802.2 Link Encapsulation00000110 = IPI-3 Slave (i.e., Master to Slave)00000111 = IPI-3 Master (i.e., Slave to Master)00001000 = IPI-3 Peer00001010 = HIPPI-FC mapping to Fibre Channel ULPs1xxxxxxx = Locally assignedNew page,Add new page 16 with Bibliography:Annex C(informative)BibliographyThe following documents are upper-layer protocols ofHIPPI-FP and are assigned ULP identifiers in 5.4.1:ANSI X3.218, High-Performance Parallel Interface -Encapsulation of ISO 8802-2 (IEEE Std 802.2) Logical LinkControl Protocol Data Units (HIPPI-LE). (Uses ULP-id =ISO 8802.2 Link Encapsulation)ANSI X3.xxx, High-Performance Parallel Interface -Mapping of Fibre Channel Signalling Protocol (HIPPI-FC).(Uses ULP-id = HIPPI-FC, which provides HIPPI physicallayer transport for Fibre Channel upper level, FC-4,protocols)ANSI/ISO 9318-3, Intelligent Peripheral Interface - Devicegeneric command set for magnetic and optical disk drives(IPI-3 Disk). (A revision to this standard uses ULP-id’s =IPI-3 Slave, IPI-3 Master, and IPI-3 Peer)ANSI/ISO 9318-4, Intelligent Peripheral Interface - Devicegeneric command set for magnetic tape drives (IPI-3 Tape).(A revision to this standard uses ULP-id’s = IPI-3 Slave, IPI-3 Master, and IPI-3 Peer)