Proposed changes to ANSI X3.222-1993— (and which have been incorporated in Rev 3.0)Proposed technical changes are preceded with (T), proposed editorial changes are precededwith (E).Rev 2.7, July 15, 1993 version - The following changes were the result of comments fromthe ISO editor, and some updated RFC numbers.1.(E) Change 4.1, last NOTE, by deleting the word "annex" in "See annex B.1 fordetails.".2.(E) Change 4.4, first entry following the NOTE, add "as described in RFC 1374 "IP andARP on HIPPI" [1]" after "..., including HIPPI-LE Address Resolution requests".3.(E) Change 4.4, other entries, by adding [n] to denote the associated entry in theBibliography.4.(E) Change Annex C, Bibliography, by the addition of "[n]" in the front of each entry tocorrespond to the new reference numbers in 4.4.5.(E) Change Annex C, Bibliography, RFC 1034 changes to "RFC 1131". The RFCnumber was incorrect.6.(E) Change Annex C, Bibliography, second entry from "RFC 826, Ethernet addressresolution protocol. (Describes a technique whereby Internet Protocol equipped hostsmay discover the media address of a destination host with a known IP address bybroadcasting a request to the IP address owner.)" to "RFC 1374, IP and ARP on HIPPI.(Describes a technique whereby Internet Protocol equipped hosts using a HIPPIcompliant interface may discover the media address of a destination host with a knownIP address.)".Rev 2.8, August 3, 1995 version - The following changes were made to support address self-discovery, and to clarify the physical nature of switch ports.7.(E) Changed the introduction by deleting the text starting "The information in thedocument..." through "Clause 5 specifies the behavior of a switch with regards to HIPPIcontrol signals" for compatibility with the ISO document.8.(E) Change clause 2. the normative reference for HIPPI-LE changes from "-199x" to "-1993".9.(T) Added HIPPI-Serial to the list of normative references in clause 2.10.(T) In 4.4, added three trial self-discovery addresses, and a paragraph of text definingtheir operation.11.(T) In 4.4, added global address FFE(hex) as "Loopback logical address". Added textto the next entry for "Unknown or unassigned address".12.(T) In 5, added the sentence: "These HIPPI ports shall conform to either the HIPPI-PHor HIPPI-Serial specifications."13.(E) Added all of B.3 in annex B describing different methods of doing address self-discovery, and an algorithm for doing it.Rev 2.9, September 26, 1995 version - The following changes were made to clarify andexpand the address self-discovery, and to add reserved addresses for switchmanagement.14.(T) In the Introduction, added a bullet about the reserved addresses. Deleted the figurefor the HIPPI documents to avoid problems with the ISO editor. Renumbered the otherfigures in the document down by one.15.(T) Add 3.1.10, a definition for "nibble".16.(E) Reordered the text of 4.4 by combining some text. Changed all of the addressesfrom binary to hexadecimal notation. Grouped addresses F90 - FBF as one item instead of three. Moved the text describing the trial self-discovery addresses from aseparate paragraph to the F90-FBF address entry.17.(T) In 4.4, removed the requirement that "a switch shall automatically provide the self-discovery address mapping, or be capable of having them loaded". Added reservedaddresses FEE and FFD.18.(T) In 5.5.2, added the fifth bullet specifying "when ... the Destination logical address isnot mapped to any physical output port".19.(T) Made major changes to annex B.3 describing the logical address self-discovery.Added a precedence for the procedures. Changed the address notation from binary tohexadecimal. Changed the description and pseudo-code to use Camp-on (before it didnot use it). Expanded the pseudo-code to include the case of connection requests"passing in the night". Expanded the pseudo-code to include a timeout. Split up andmoved the explanatory text closer to the pseudo-code entries. Broke the connectionafter each trial.Rev 3.0, January 24, 1996 version - The following changes were made to the address self-discovery pseudo-code, and to add cautions about different clock frequencies inimplementations.20.(E) On the front cover, the name of the secretariat was updated to their new name, i.e.,ITI.21.(T) Changed the last paragraph and pseudo-code in B.3.5.3 to check for a host directlyconnected to another host without an intervening switch. The change shows up in Rev3.0, in the last three paragraphs, and associated pseudo-code, of B.3.5.3.22.(T) Added B.4 with cautions about different CLOCK frequencies affecting the CONNECTand READY signals. This is essentially the same text that is in HIPPI-Serial D.1.2 andD.1.3.